
System PSLC (vms 4.3)

Username: SHADOW
Password: 
        Welcome to VAX/VMS Version 4.3
       University of Wisconsin - Madison
         Physical Sciences Laboratory 

VAX C was upgraded to version 2.2.
Top Drawer plots can now be made on the new LN03S laser printer!
Read the Bulletin for more information.

    Last interactive login on Saturday, 14-JUN-1986 12:29
    Last non-interactive login on Tuesday, 25-FEB-1986 21:46

You are logged into _RTA1:



Graphic device [ e.g. TTB3: ] : tt:

All logical names command defined.

Enter $GO to activate SHADOW.
Enter HELPSHA for help.
Type NEWS for recent modifications.: 

$ go


  :::::::  :::    ::            :::    :::::::        :::::     :::  ::  ::
 ::::::::  :::    ::           ::::    ::::::::      :::::::    :::  ::  ::
:::        :::    ::          ::: :    :::   :::    :::    ::   :::  ::  ::
:::        :::    ::         ::: ::    :::    ::    :::    ::   :::  ::  ::
 :::::::   :::::::::        :::  ::    :::    ::    :::    ::   :::  ::  ::
  :::::::  :::::::::       :::   ::    :::    ::    :::    ::   :::  ::  ::
       ::  :::    ::      :::    ::    :::    ::    :::    ::   :::  ::  ::
      :::  :::    ::     :::     ::    :::   :::    :::   :::   ::: ::: :::
::::::::   :::    ::    :::      ::    ::::::::      :::::::     :::::::::
:::::::    :::    ::   :::       ::    :::::::        :::::       ::: :::




VERSION     86.4                                                19 JAN 1986




Hit <RETURN> when ready: 







                            S H A D O W


Commands Available at this level:

HELP              More informations on the following commands
INIT              Defines scratch directories and set default to scratch
MENU              Begins the process of defining an Optical System
TRACE             Starts the tracing of an Optical System from a specified
                  source file
SOURCE            Generates a source file
EXIT              Returns to DCL







Shadow:: source

SOURCE selected. Begin procedure.

This procedure generates a SOURCE for SHADOW.
Mode selected [ ? <ret> for HELP ] ? : ?
 Enter : 
MENU       for screen-driven menus
PROMPT            prompted session
NAMELIST     file-oriented session

This procedure generates a SOURCE for SHADOW.
Mode selected [ ? <ret> for HELP ] ? : prompt
Call to INPUT

---------------------------------- S H A D O W  -------------------------------
Jan 1986                                         F.Cerrina        ECE - UW     

Defining source : 
When prompted for a yes/no answer, you may enter:
for   YES  answer      Y, 1
for   NO   answer      anything else




Do you want a verbose [ 1 ] or terse [ 0 ] output ?
0
------------- SOURCE SPECS ------------------
Source modelling type [ 0-5 ] ? 
0
How many rays [ 1 - 5 000 ] ? 
1000
Seed [ odd, 1000 - 1 000 000 ] ? 
10101011
X-Z plane source type [ 0-3 ] ? 
3
Sigma along X ? 
.2
            Z ? 
.2
Source Depth [ 1-4 ] ? 
1
Source Angle Distribution [ 1-6 ] ? 
3
Horizontal half-divergence [ (+)x, rads ] ? 
.001
                           [ (-)x, rads ] ? 
.001
Vertical                   [ (+)z, rads ] ? 
.001
                           [ (-)z, rads ] ? 
.001
Vertical sigma [ rads ] ? 
.0001
Horizontal              ? 
.0001
Do you want a Photon energy [ Y/N ] ? 
Y
Energy distribution [ 1-3 ] ? 
1
Photon Energy [ 0 ] or Angstroms [ 1 ] ? 
1
Wavelength [ A ] ? 
4600
Do you want to store the optical paths (OPD) [Y/N] ?
N
Do you want to generate the A vectors (electric field) [Y/N] ?
N
Exit from INPUT_SOURCE


Generated          250 rays out of         1000
                   500
                   750
                  1000
Exit from SOURCE
SOURCE => Source has been succesfully generated.

SOURCE procedure completed.

Shadow:: ?


 ? Command not recognized ? 

 Legal commands are: 
EXIT     MENU     TRACE      SOURCE     HELP    INIT

Shadow:: TRACE


Ray Tracing Selected. Begin procedure.


Mode selected [ ? <ret> for HELP ] ? : PROMPT
PROMPT selected.
Call to RESET
Exit from RESET


Mode selected is: 
PROMPT                                                                          
Options: to start anew                 [ 0 ] 
            to restart from a given OE [ 1 ] 
Then ? 
0
Call to INPUT_OE



---------------------------------- S H A D O W  ------------------------------- 
Jan 1986                                         F.Cerrina        ECE - UW      

Defining Optical Element:  1
Continue ? [ ^Z or %EXIT to terminate OS ] 
Y
When prompted for a yes/no answer, you may enter:
for   YES  answer      Y, 1
for   NO   answer      anything else




Do you want a verbose [ 1 ] or terse [ 0 ] output ?
0

Optical Element definition:
Incidence Angle ? 
0
Source Distance ? 
1000
Reflection Angle? 
180
Image Distance  ? 
1
Reflector [ 0 ] or refractor [ 1 ] ? 
1
Enter the index of refraction in OBJECT space:
Object space: 
1
Enter the index of refraction in IMAGE space:
Image space: 
1.5
Mirror surface [ 1-9] ? 
1
Do you want to specify the mirror parameters ?
Y
Is the mirror Cylindrical ? 
0
Are we dealing with a Grating ? 
0

Are we dealing with a crystal [ Y/N ] ? 
0
Is the mirror convex [ Y/N ] ? 
Y

Orientation Angle [ Alpha ] ? 
0

Mirror Dimensions finite [ Y/N ] ?
0

Spherical Mirror Radius ? 
1000

Do you want to move the Source [ Y/N ] ? 
0
   
Do you want to move the mirror itself [ Y/N ] ? 
0
Rippled surface [ Y/N ] ? 
0

Any screens in this OE [ Y/N ] ? 
0

Slit at continuation plane [ Y/N ] ? 
0
Extra Image plates [ Y/N ] ? 
0
File containing the source array ? 
BEGIN.DAT
Exit from INPUT
Do you want to modify some inputs ? 
0
Tracing optical element #            1
Call to SETSOUR
Exit from SETSOUR
Call to IMREF
Exit from IMREF
Call to OPTAXIS
Exit from OPTAXIS
Call to MSETUP
Exit from MSETUP
Call to RESTART
Exit from RESTART
Call to MIRROR
Exit from MIRROR
Call to IMAGE
Exit from IMAGE
Call to RESET
Exit from RESET

Do you want to change input mode ? 
0
Call to INPUT_OE
---------------------------------- S H A D O W  ------------------------------- 
Jan 1986                                         F.Cerrina        ECE - UW      

Defining Optical Element:  2
Continue ? [ ^Z or %EXIT to terminate OS ] 
Y
When prompted for a yes/no answer, you may enter:
for   YES  answer      Y, 1
for   NO   answer      anything else




Do you want a verbose [ 1 ] or terse [ 0 ] output ?
0

Optical Element definition:
Incidence Angle ? 
0
Source Distance ? 
4
Reflection Angle? 
180
Image Distance  ? 
1000
Reflector [ 0 ] or refractor [ 1 ] ? 
1
Enter the index of refraction in OBJECT space:
Object space: 
1.5
Enter the index of refraction in IMAGE space:
Image space: 
1
Mirror surface [ 1-9] ? 
1
Do you want to specify the mirror parameters ?
1
Is the mirror Cylindrical ? 
0
Are we dealing with a Grating ? 
0
Are we dealing with a crystal [ Y/N ] ? 
0
Is the mirror convex [ Y/N ] ? 
0

Orientation Angle [ Alpha ] ? 
0

Mirror Dimensions finite [ Y/N ] ?
0

Spherical Mirror Radius ? 
1500

Do you want to move the Source [ Y/N ] ? 
0
Do you want to move the mirror itself [ Y/N ] ? 

Rippled surface [ Y/N ] ? 


Any screens in this OE [ Y/N ] ? 


Slit at continuation plane [ Y/N ] ? 

Extra Image plates [ Y/N ] ? 

Exit from INPUT
Do you want to modify some inputs ? 

Tracing optical element #            2
Call to SETSOUR
Exit from SETSOUR
Call to IMREF
Exit from IMREF
Call to OPTAXIS
Exit from OPTAXIS
Call to MSETUP
Exit from MSETUP
Call to RESTART
Exit from RESTART
Call to MIRROR
Exit from MIRROR
Call to IMAGE
Exit from IMAGE
Call to RESET
Exit from RESET

Do you want to change input mode ? 

Call to INPUT_OE


---------------------------------- S H A D O W  -------------------------------
Jan 1986                                         F.Cerrina        ECE - UW     

Defining Optical Element:  3
Continue ? [ ^Z or %EXIT to terminate OS ] 
