# EXODUS

## Function

Manipulate and overplot multiple sets of data form ASCII files (optimized for SPEC files):

1. It loads a SPEC file and user can select, view, interpolate, average, and perform operations with data from multiple scans. It also accepts MCS SPEC scans. Hete the XCol=1 means channel numbet and XCol=2 means Energy (using calibration from spec file).

2. It also loads data from ASCII files and from other XPlot windows.

3. It allows to export the selected data set from one or many SPEC files into files of different types (Spec/Scan,Spac/Mesh, etc.)

4. It contains some tools to convert and operate with lists of Spec/MCA files.

## Documentation

- application doc