               Description of the input parameters for XTUBE_W:
               ================================================


VOLTAGE:     anode voltage in kiloVolts (in the 30-140 interval)
VOLTAGE RIPPLE: RMS value in %
AL FILTER: Al filtration: layer thickness in mm

