----- header of fufifa.pro extracted on: Wed Mar  5 17:24:02 2008

----- Documentation for /scisoft/xop2.3/src_idl/wutil/fufifa.pro -----

                         ===============================
                         = Functional Fitting Facility =
                         ===============================

 FuFiFa 


 Fufifa is an application to fit interactively a SEVERAL spectra to a FUNCTION.

 The goal is to provide with a point-and-click application for fitting many 
 data sets (usually imported from a SPEC file, that can be prepared with 
 Xop/EWxodus) with a user-defined function. 

 The function can be built interactively using a set of components (straight 
 line, polynomial, peaks (gaussian, lotentzian and pseudovoigt), steps (error 
 function and arc tangent) or any user-define function). 

 The application allows to fit simultaneously several data sets and to
 refine individually the fits. A plot of the fitted parameters and chi square 
 versus the data set index can help to estimate the quality of the fits. 

 To operate with fufifa follow the following steps:

 1) Start the application by either: 

 i) Start xop and from the Xop->Tools->FuFiFa, This will create the fufifa 
    window.
 ii) Enter "xop fufifa" at the unix prompt

 2) Import your data.
   Press the load button in the data sector (top right of the main window).
   You should select a file (SPEC type) which has been previously "cleaned".
   "Cleaned SPEC file" means that:
     i) you have removed the unwanted scans (only kept those used for fitting)
     ii) Each scans has ONLY two or three columns
         The first one is the abscissas X
         The second one is the ordinates Y
         The third (optional) one contains the errors of Y. The errors used for
            the fit are defined in the Fit->Preferences menu item. 
    You can use the EXODUS application (available in the XOP/XAID-XAFS toolbox)
         for this purpose (i.e., cleaning your SPEC file).

    Example: Using the file cat3.spec I
             extracted (using EXODUS) the scans [82,83,92,93,111,112 and 113] 
             I used column 1 for X and column 16 for Y. The result was 
             written to file exodus.spec. This file was imported into fififa. 
             Then I selected all scans (by pressing ctrl-click iteratively or 
             doing multiple selection with shift-click). 
             The result of these operations are in Fig1.

 3) Define your model:
    Using the bottom sector of your fufifa window, I defined a function 
    consisting in a step function (errorF) and a lorentzian peak. For this 
    I clicked "Add function" twice, one for each functional component. 
    I did not adjust the input parameters. 

    First I select my first scan (clicking on the list at the top right sector).
    The meaning of the small buttons for each model line are the following:
    "x" : removes the model line
    "G" Get the guess values (using the mouse for peaks and straight lines)
    Each parameter can be modified directly by enteing a new number, or by 
    pressing:
    "F" Fixes this parameter (not changed during the fit)
    "B" Edit parameter boundaries

 4) First attempt to fit.
    If you press "**Fit**" you fit the function parameters to data. 
    Then you can press "Copy Pars To All DataSets" that copies the fitted 
    values for the first scan to the rest of scans. 

    If you want to fit all spectra, just make a multiple selection and press 
    the fit button. Then you can select individual scans to see better the 
    results.
    Perhaps some scans are not well fitted. You can select by hand the guess
    parameters and fit again. 

 5) Refinement of the fit. 
    You can preprocess the data using the "Data" menu items to:
      i) perform some operation (like normalization).
      ii) Cut unwanted data and redefine your interval. Use it to remove 
          points of the pre-edge and the incomplete last oscillation. 
      iii) Substract a linear background (not needed in this case). 

      After doing that, I added two more lorentzian peaks. I got results shown
      in Fig4. Much better!

      iv) You can ignore a part of the data for fitting purposes bu using the
      option "Include [a,b] and/or exclude {a,b} regions"

 6) Visualizing and saving results:
     By pressing "Pars vs Data Sets" you can mahe plots of the parameters and 
     the reduced Chi square versus the scan number. 
     This permits you to see if there are drastic changes in some parameters.  

     In order to save the full information, you can use FuFiFa->Save as... 
     It will
     create a SPEC-type file with all scans, error used, and models. 
     In the scan header you can find the information on the fitted parameters 
     and chi**2. The last scan (numbered 1000) contains the variation of 
     the parameters versus the scan index. 
     Of course, you can use Xplot to view this resulting file. 
     This file can be reloaded in FuFiFa.



  Non Interactive use:
	; load ASCII Files
	fufifa,Parent=p
	fufifa_loadfile,p,isel=0 ; import ascii file (start browser)
	fufifa_loadfile,p,isel=0,File='CuFoilRef.txt',append=0 ; import ascii 

	; load SPEC Files
	fufifa_loadfile,p,isel=1,File='fufifa.spec',Append=0



 Some functionality already implemented
 - Load components of the function from an external (customizable) file
 - Access to boundaries of parameters for the fit
 - "Expert" mode (do not show information windows)
 - Integrated in xplot and in xop 
 - Prints single or multiple plots
 - Exports fitting data to a Excel file

 ToDo:
 - Allow MCI inputs
 - Abort button (when fitting...)
 - Customize colors
 - Polynomial inputs from mouse
 - Interactive help

  COPYRIGHT:
 	FUFIFA belongs to XOP package and it is distributed within XOP.
 	PLEASE REFER TO THE XOP COPYRIGHT NOTICE
 
  REFERENCE:
 	Published calculations made with XOP should refer:
 
 	M. Sanchez del Rio and R. J. Dejus 
         "Status of XOP: an x-ray optics software toolkit"
         SPIE Proceedings Vol. 5536 (2004) pp.171-174
 
         http://dx.doi.org/10.1117/12.560903
 
  LAST MODIFICATION: srio@esrf.eu 2008-02-01
 
 HISTORY:
 
 srio@esrf.fr 7 December 2001
 Modified:
     2003/12/09 srio@esrf.fr Fix an incompatibility problem for IDL >=5.6
     2006/03/02 srio@esrf.fr Allows non-interactive use:  FUFIFA_LOADFILE
     2006/10/02 srio@esrf.fr Many upgrades. Version 1.00
     2006/10/10 srio@esrf.fr Direct export to FuFiFa
     2006/11/07 srio@esrf.fr Debug load file with model.



 PRO fufifa_loadfile,parent,isel=isel,Dialog_Parent=dialog_Parent,file=file

 06-03-02 srio@esrf.fr

 isel: 0 ASCII FILE(S)
 isel: 1 SPEC CLEANED FILE
 isel: 2 DATA block (use Title keyword)


