# XINPRO

## Function

calculate perfect crystal reflectivity. xinpro calculates the diffracted and transmitted profiles in reflection (Bragg) and transmission (Laue) geometries for plane perfect crystals.

NOTE: This is an standalone program developed at the ESRF optics group. XOP developers recommend to use xcrystal, as it has a wider functionality and uses DABAX files.

## Documentation

- application doc

- input parameters

- See also: X-ray Optics

## Technical aspects

- Bug: The Debye-Waller model diverges for zero Kelvin.